|  |  |  |  |
| --- | --- | --- | --- |
| Capacitor 22 uF    (x3) | Capacitor 2.2 uF | Capacitor (x2) 0.1 uF    (x2) | IC TLC555 |
| Diode (1 amp) 1N4004 | Diode small 1N4148 | LED – Green | 9V battery clip |
| Resistor 10 ohm 1W | Resistor 330 ohm ¼ W    orange-orange-brown | Resistor 1K ohm ¼ W    brown-black-red (x3) | Resistor 10K ohm ¼ W    brown-black-orange |
| Switch DP3T | Pot, 100 K ohm, 9mm size | Speaker, 1/2W, 16 ohm | PCB |
| Hookup wire | Output connector ¼” phone  Amphenol | Alternate output connector (you will have only one of these two) |  |